# Adafruit AHTX0 (AHT10 & AHT20) [![Build Status](https://github.com/adafruit/Adafruit_AHTX0/workflows/Arduino%20Library%20CI/badge.svg)](https://github.com/adafruit/Adafruit_AHTX0/actions)

This is the Adafruit AHT10+AHT20 Humidity and Temperature Sensor library for Arduino

Tested and works great with the Adafruit AHT20 Breakout Board
[<img src="assets/board.png?raw=true" width="500px">](https://www.adafruit.com/products/)


This chip uses I2C to communicate, 2 pins are required to interface

Adafruit invests time and resources providing this open source code, please support Adafruit and open-source hardware by purchasing products from Adafruit!

# Dependencies
* [Adafruit_BusIO](https://github.com/adafruit/Adafruit_BusIO)
* [Adafruit_Sensor](https://github.com/adafruit/Adafruit_Sensor)

# Contributing

Contributions are welcome! Please read our [Code of Conduct](https://github.com/adafruit/Adafruit_AHT10/blob/master/CODE_OF_CONDUCT.md>)
before contributing to help this project stay welcoming.

## Documentation and doxygen
Documentation is produced by doxygen. Contributions should include documentation for any new code added.

Some examples of how to use doxygen can be found in these guide pages:

https://learn.adafruit.com/the-well-automated-arduino-library/doxygen

https://learn.adafruit.com/the-well-automated-arduino-library/doxygen-tips

Written by ladyada for Adafruit Industries.
BSD license, check license.txt for more information
All text above must be included in any redistribution

To install, use the Arduino Library Manager and search for "Adafruit AHTX0" and install the library.
